Dear Prof. Brady,

During hand augering, we didn't detect ground water table at all sites,

I just estimate water table from p.w.p. graphs, considered with our drilling data (but these are not very near)

Akemi E.S. -2.3 m

Hinode E.S. -3.0 m

Hinode Minami E.S. -2.3 m

Hosoyama -4.1 m

Irifune N.S. -1.8 m

Takasu Cyu-ou Park -2.5 m

Takasu Kaihin Park -2.9 m